**PETROL COKE - Specifications**



**Fuel Grade Raw Petrol Coke**

(Low Sulphur)

|  |  |  |  |
| --- | --- | --- | --- |
| **Specification** **Sl No**  | Parameter  | **Unit**  | **Value**  |
| **1**  | Moisture content (As received)  | % Mass  | 8 max  |
| **2**  | Ash ( ADB )  | % Mass  | 1 max  |
| **3**  | Volatile Matter ( ADB )  | % Mass  | 8 min  |
| **4**  | Fixed Carbon (Calculated)  | % Mass  | 87 min  |
| **5**  | Total Sulphur ( ADB )  | % Mass  | 3.5 to 5 max  |
| **6**  | Hargrove Grindability Index (HGI)  |  35-60 min.  |
| **7**  | Gross Calorific Value (GCV)( ADB )  | Kcal/Kg  | 8200 min  |